IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "2018_01"
Time stamp: "2020-07-13T14:16:32"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.0.0.376 - Exporter 21.0.0.376 - Default UI"
Application: "Autodesk Revit 2021 (DEU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (DEU)"

People and organizations
  Person "c.hort" of Organization (no name given)
  Owner history of Person "c.hort" of Organization (no name given) | application "Autodesk Revit 2021 (DEU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (DEU)" | change NOCHANGE | created 1594642578 (2020-07-13T12:16:18Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  CURRENCY: EUR
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "2018_01" | phase "Projekt Status"
  IFCSITE "Default" | latitude 48° 8′ 15.359802″ | longitude 11° 34′ 47.783432″ | elevation above sea level 519.
    contains 1 element
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Familie1:Norm" | object type "Familie1:Norm" | names: "Familie1:Norm:2409400" | material: materials ("RAL 9005", "Glatt - weiß") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Abhängigkeiten, Abmessungen

Types
  IFCBUILDINGELEMENTPROXYTYPE "Familie1:Norm" | 1 occurrence | material: "RAL 9005" | property sets: Abhängigkeiten, ID-Daten, Modelleigenschaften, Sonstige, Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation

Property sets
  ID-Daten | properties | on 1 object (1 IFCSITE)
    Gebäudebezeichnung = "" (IFCTEXT)
    Unternehmensbeschreibung = "" (IFCTEXT)
    Unternehmensname = "" (IFCTEXT)
    Verfasser = "" (IFCTEXT)
  ID-Daten | properties | on 1 type object
    Baugruppenbeschreibung = "" (IFCTEXT)
    Baugruppenkennzeichen = "" (IFCTEXT)
    Beschreibung = "Arres 3.0 Premium (325Wp)" (IFCTEXT)
    Codename = "" (IFCTEXT)
    Hersteller = "Solarmarkt GmbH" (IFCTEXT)
    Modell = "Arres 3.0 Premium (325Wp)" (IFCTEXT)
    OmniClass-Nummer = "" (IFCTEXT)
    OmniClass-Titel = "" (IFCTEXT)
    Typname = "Norm" (IFCTEXT)
    URL = "https://www.solarmarkt.ch/de/arres30premium/102603171" (IFCTEXT)
  Sonstige | properties | on 1 object (1 IFCSITE)
    Auftraggeber = "Bauherr" (IFCTEXT)
    Kategorie = "Projektinformationen" (IFCLABEL)
    Projektadresse = "Projektadresse" (IFCTEXT)
    Projektausgabedatum = "Projekt Datum" (IFCTEXT)
    Projektname = "" (IFCTEXT)
    Projektnummer = "2018_01" (IFCTEXT)
    Projektstatus = "Projekt Status" (IFCTEXT)
    Verfasser Firma 1 = "AUTODESK GmbH" (IFCTEXT)
    Verfasser PLZ Ort = "Ort" (IFCTEXT)
    Verfasser Strasse = "Adresse" (IFCTEXT)
    Verfasser Telefon = "Telefon" (IFCTEXT)
    Verfasser URL = "www.Autodesk.de/BIM" (IFCTEXT)
    Verfasser eMail = "E-Mail" (IFCTEXT)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Familie = "Familie1: Norm" (IFCLABEL)
    Familie und Typ = "Familie1: Norm" (IFCLABEL)
    Kategorie = "Allgemeines Modell" (IFCLABEL)
    Typ = "Familie1: Norm" (IFCLABEL)
    Typ-ID = "Familie1: Norm" (IFCLABEL)
  Sonstige | properties | on 1 type object
    Familienname = "Familie1" (IFCTEXT)
    Kategorie = "Allgemeines Modell" (IFCLABEL)
  Text | properties | on 1 object (1 IFCSITE)
    Bauherr = "AUTODESK" (IFCTEXT)
    Baustellenort = "BAUORT" (IFCTEXT)
    Baustellenstraße = "BAUSTRASSE 1" (IFCTEXT)
    Einlagezahl = "123-45" (IFCTEXT)
    Gerichtsbezirk = "GERICHTSBEZIRK" (IFCTEXT)
    Grundstücksnummer = "GR" (IFCTEXT)
    Katastralgemeinde = "KG" (IFCTEXT)
    Kundenadresse = "KUNDENSTRASSE 1" (IFCTEXT)
    Kundenort = "KUNDENORT" (IFCTEXT)
    Kundentelefon = "0000-00000-1" (IFCTEXT)
    Kundenzusatz = "KUNDENZUSATZ" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Norm" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Solarmarkt GmbH" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Norm" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    System = "Indach" (IFCLABEL)
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Keine" (IFCTEXT)
    Höhe von Ebene = 0. (IFCLENGTHMEASURE) [METRE]
    Versatz von Host = 0. (IFCLENGTHMEASURE) [METRE]
    Verschieben mit umliegenden Elementen = FALSE (IFCBOOLEAN)
  Abhängigkeiten | properties | on 1 type object
    Vorgabe-Ansicht = 0. (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Fläche = 2.45571578921423 (IFCAREAMEASURE) [SQUARE_METRE]
    Volumen = 0.0110434269880893 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Phasen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase erstellt = "Phase 2" (IFCLABEL)
  Modelleigenschaften | properties | on 1 type object
    Backsheetfarbe/EVA = "schwarz" (IFCTEXT)
    Breite = "1060 mm" (IFCTEXT)
    Gewicht = "22,70 kg" (IFCTEXT)
    Homepage = "https://www.arres.ch/" (IFCTEXT)
    Höhe = "20 mm" (IFCTEXT)
    Kabellänge = "900 mm" (IFCTEXT)
    Kurzschlusstrom (Ik) = "10,05 A" (IFCTEXT)
    Leerlaufspannung (Uoc) = "41,11 V" (IFCTEXT)
    Leistung = "325 Wp" (IFCTEXT)
    Leistungsgarantie = "25 Jahre" (IFCTEXT)
    Leistungstoleranz = "-0/+5" (IFCTEXT)
    Länge = "1691 mm" (IFCTEXT)
    MPP-Spannung (Umpp) = "33,29 V" (IFCTEXT)
    MPP-Strom (Impp) = "9,78 A" (IFCTEXT)
    Max. Schneelast = "9 kN" (IFCTEXT)
    Max. Systemspannung = "1000 V" (IFCTEXT)
    Max. Windsog = "2,40 kN" (IFCTEXT)
    Modulwirkungsgrad = "19,45 %" (IFCTEXT)
    Produktgarantie = "10 Jahre" (IFCTEXT)
    Rahmenfarbe = "schwarz" (IFCTEXT)
    Steckertyp = "Stäubli MC4" (IFCTEXT)
    System = "Indach" (IFCTEXT)
    Temperaturkoeffizient (TKp) = "-0,38 %/K" (IFCTEXT)
    Trafo erfoderlich = "nein" (IFCTEXT)
    Zelltyp = "Momokristallin" (IFCTEXT)